tab Input linearization

# Input linearization

Segmental linearization function allows to insert individual input user characteristics into intelligent transmitters (Sensor).

The above picture presents a user interface window. It contains the following subareas (from the left):

- Values table
- Graphic representation of values

- The Y-axis
- input (mV)
- The X-axis
- output (mV)

- buttons:

- Read from a device reads current linearization table from a transmitter.
- Write to a device writes a linearization table in a transmitter.
- New - creates a new linearization table. The table is filled up with default values.
- Open imports a table from file.
- Save exports a table to file.
- Insert adds a row to a table.
- Delete removes a row from a table.
- Sort - sorts table values ascending. The program requires that each point has a value (pv(mA) and a value ) larger than the previous one.

Note: To activate input linearization, input type must be set to Users table, as show below