# Transmitter configuration

Note: All functions described in this section require previous transmitter identification in the network by the transmitter search tool!

## New transmitter

The option is run by:

> - Menu->File->New transmitter.

Choosing this option will configure the program for operation with a selected type of transmitter without the need to connect a real transmitter.
It allows to do the following:

- Create a configuration template for a given type of transmitters.
- Preview of transmitter configurations saved in file.

## Reading transmitter configuration

The program allows to run this function in the following ways:

> - The button located on the taskbar,
> - Menu->Transmitter->Read configuration.

If you choose this function, all transmitter parameters will be read.

## Save configuration to a transmitter

The program allows to run this function in the following ways:

> - The button located on the taskbar,
> - Menu->Transmitter ->Enter configuration.

If you choose this function, all transmitter parameters will be saved.

## Import transmitter configuration from file

The program allows to run this function in the following ways:

> - The button located on the taskbar,
> - Menu->File->Import configuration.

This function allows to import previously exported transmitter configuration. Note: Only editable parameters are imported. The parameters, which cannot be edited (and therefore, are not saved in file) have greyed-out background and are not imported to a transmitter.

The basic function of that option is to import parameters to a transmitter on the basis of a previously created configuration template. Below, you can find an example of template creation procedure based on parameters of a selected transmitter, and then import of the prepared data to another transmitter:

Template preparation

- First search for a transmitter, which will be a template model,
- Then, choose Export configuration to save the transmitter parameters to file (template),
- Disconnect the transmitter from the network.

Import the template into another transmitter

- Connect the second transmitter, to which template parameters will be imported (both transmitters must have the same basic range),
- Search for a transmitter,
- Import configuration from file (Menu->File->Import configuration),
- After importing data from file, some parameters can be changed e.g. sensor number,
- Upload new transmitter configuration by tool Save configuration to a transmitter

## Export transmitter configuration to file

The program allows to run this function in the following ways:

> - The button located on the taskbar,
> - Menu->File->Export configuration.

This function allows to save selected transmitter parameters to file.
Note: Only editable parameters are imported. The parameters, which cannot be edited (and therefore, are not saved in file) have greyed-out background.

## Generate transmitter configuration report

The program allows to run this function in the following ways:

> - The button located on the taskbar,
> - Menu->Transmitter->Generate report.

A generated configuration report can be printed out or saved in various file formats.