tab Basic parameters

# Basic parameters

It contains transmitter basic parameters.

- Unit
- Current unit of PV (first process variable).
- Transfer function

- Linear
- Root
- Square
- Special
- if enabled, a transmitter operates on the basis of characteristics defined in the operation: Linearization or Output linearization for Li24

- Lower, upper sensor limit
sensor limits.
- Lower, upper range value
- Start and end of an measuring range. The limits for the start and end of measuring range are limited by sensor limits.
- Minimal range width
- Minimal width of the setting range.
- Damping value
- Transmitter’s time constant (damping time).

Content of fields, in which value can be entered, can be inserted to the transmitter with a command Write.The command Read allows to read only those parameters, which are shown in the above window. To read all transmitter parameters, you should use the command Read configuration.