tab Basic functions

# Basic functions

This operation displays a basic functions window.

Available functions allow the following operations:

- Change of range set-value,
- Direct current mode in the line,
- Transmitter reset
- Soft transmitter reset.
- Configuration change flag
- It allows to delete hardware configuration change flag. The flag is set in transmitter memory at each transmitter parameters change.
- Analog output calibration.
- Zeroing
- Zeroing of the first process variable. It does not apply to absolute pressure transmitters.
- Change of time constant
- Allows reading or changing transmitter time constant.