tab Transmitter parameters

# Transmitter parameters

It contains additional transmitter parameters. The window layout depends on a transmitter type. Below you can see a window containing settings of one of the transmitters.

- Long tag
- a message field for any content, cannot be longer than 24 characters.
- Inflection point
- relates to root characteristics. The range percentage from which this characteristics is enabled. Below this value, the transmitter operates on the basis of own characteristics (cubic function).
- Product code
.

Restore factory settings:

- If any of the following operations is carried out incorrectly, the program allows to restore factory settings:
- Undo zero calibration
- concerns zeroing operation run by Operations->Basic functions->Zeroing.
- Undo sensor calibration
- concerns the operation transmitter input signal calibration.
- Undo analog output calibration
- concerns the operation analog output calibration.

Analog output configuration:

- Operation mode
- alarm limits depend on a selected mode:

- Normal
- standard alarm limits.
- Namur
- Namur-compliant alarm limits.

- Alarm current
- define current to be set in case of an alarm::

- High
- 22,0 mA current will be set.
- Low
- 3,8 mA current will be set.

- Output operation limit
- a read-only parameter, visible only for some transmitters.
- Alarm at
- select which module errors activate the transmitter’s alarm:

- HART error
- ADC error
- EEPROM error
- Oscillator error
- error DS33

- Filtration
- Variable connected with input sampling frequency.

Limits:

- Pressure
- Transmitter compensation limits
- Temperature
- permissible operating temperature.

Version information - software and transmitter electronics versions.

Content of fields, in which value can be entered, can be transfered to the transmitter with a command Write.
The command Read allows to read only those parameters, which are shown in the above window.
To read all transmitter parameters, you should use the command Read configuration.