tab Write protection

# Write protection

The transmitter allows to block the possibility of changing its parameters by unauthorized users. With this tool you can manage transmitter access passwords and the lock status.

Lock status
- Unblocked
- access to transmitter settings changes is unprotected.
- Blocked
- access to transmitter settings changes is protected.
- Blocked(spec)
- access to transmitter settings changes is protected. This option is available for MID transmitters only.

To change the lock settings, you must define the lock status, and then click a Set button. The program will ask for an access code currently entered into a transmitter. Password for brand-new transmitters is 00-00-00-00.

To change a transmitter lock password, choose the Change password button.