# Change of adjusted range by entering numbers

To change the transmitter’s adjusted range, perform the following operations:

1. If a transmitter was not found in the network, you must search for it.
2. Go to Basic parameters tab.
3. Adjust unit.
4. Set start and end of the adjusted range. Permissible values are limited by the basic range and minimal range width.
5. Save changes in a transmitter by clicking Enter.

See also:
Set range with assigned values.