tab Description

# Description

It contains auxiliary parameters, which enable to set own description.

Marker - eight alphanumeric characters, which may be used for transmitter description e.g. Id of place in which it is installed.
Description – sixteen alphanumeric characters for user comment.
Message – thirty two alphanumeric characters, which may be used depending on user’s needs.
Date – date in the format dd-mm-yy. Number of days from 1 to 31. Number of months from 1 to 12. Maximum value of year is 2155.

Parameters can be transferred to the transmitter with a Write parameters command. The command Read parameters allows to read only those parameters, which are shown in the above window. To read all transmitter parameters, you should use the command Read configuration.