tab Output linearization

# Output linearization

Segmental linearization function (output track) allows to insert individual output user characteristics into intelligent transmitters.

The above picture presents a user interface window. It contains the following subareas (from the left):

- Values table
- Graphic representation of values

- The Y-axis
- input (%)
- The X-axis
- output (mA)

- buttons:

- Read from a device – reads current linearization table from a transmitter.
- Write to a device – writes a linearization table in a transmitter.
- New - creates a new linearization table. The table is filled up with default values.
- Open – imports a table from file.
- Save – exports a table to file.
- Insert – adds a row to a table.
- Delete – removes a row from a table.
- Sort - sorts table values ascending. The program requires that each point has a value (pv(mA) and a value ) larger than the previous one.

Note: To activate transmitter’s linearization, conversion characteristics must be set to User’s function, as show below.

The procedure of characteristics change is described inConversion characteristics change.