; Windows Modem Setup File
; Copyright (c) 2002 Atoll Vitebsk
; Manufacturer: Atoll Vitebsk, Inc. (DVINA)

[Version]
LayoutFile=layout.inf, layout1.inf, layout2.inf
CatalogFile=mdmgen.cat
Signature="$CHICAGO$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%Mfg%
DriverVer = 09/09/2005,1.0.0.5     ; Версия драйвера 1.0.0.5

[ControlFlags]
ExcludeFromSelect=SERENUM\DVL0001,SERENUM\DVL0002,SERENUM\DVL0003,SERENUM\DVL0004

[Manufacturer]
%Mfg% = Models

[Models]
%Modem01PNP% = Modem01, SERENUM\DVL0001 ; DVINA Light external PnP
%Modem02PNP% = Modem01, SERENUM\DVL0002 ; DVINA Light USB
%Modem03PNP% = Modem01, SERENUM\DVL0003 ; DVINA Easy external PnP
%Modem04PNP% = Modem01, SERENUM\DVL0004 ; DVINA Easy USB
%Modem01% = Modem01,DVL0001X            ; DVINA Light external

; Installation sections

[Modem01]
AddReg = All, MfgAddReg, Modem01.AddReg, External


; AddReg sections

[Modem01.AddReg]
HKR,, Properties, 1, 80,01,00,00, FF,00,00,00, 00,00,00,00, 07,00,00,00, 0F,00,00,00, 10,03,00,00, 00,C2,01,00, 40,83,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,C2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00

[Strings]
Mfg = "Atoll Vitebsk, Inc."

Modem01PNP = "DVINA Light C-32 External Plug & Play"
Modem02PNP = "DVINA Light C-32 USB"
Modem03PNP = "DVINA Easy C-32 External Plug & Play"
Modem04PNP = "DVINA Easy C-32 USB"
Modem01    = "DVINA Light C-32 External"

; Common sections

[All]
HKR,,FriendlyDriver,,unimodem.vxd
HKR,,DevLoader,,*vcomm
HKR,,PortSubClass,1,02
HKR,,ConfigDialog,,modemui.dll
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR, Init, 1,, "ATE0Q0V1<cr>"
HKR, Responses, "<cr><lf>OK<cr><lf>", 1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00

[EXTERNAL]
HKR,, DeviceType, 1, 01

;[INTERNAL]
;HKR,, DeviceType, 1, 02

[MfgAddReg]
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Init, 2,, "ATE0Q0V1<cr>"
HKR,, Reset,, "ATZ<cr>"
HKR, Monitor, 1,, "ATS0=0<cr>"
HKR, Monitor, 2,, "None"
HKR, Hangup, 1,, "ATH<cr>"
HKR, Answer, 1,, "ATA<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ""
HKR, Settings, SpeakerVolume_Low,, "L0"
HKR, Settings, SpeakerVolume_Med,, "L2"
HKR, Settings, SpeakerVolume_High,, "L3"
HKR, Settings, SpeakerMode_Off,, "M0"
HKR, Settings, SpeakerMode_Dial,, "M1"
HKR, Settings, SpeakerMode_On,, "M2"
HKR, Settings, SpeakerMode_Setup,, "M3"
HKR, Settings, FlowControl_Hard,, "&H1&R2&I0"
HKR, Settings, FlowControl_Off,, "&H0&I0&R1"
HKR, Settings, FlowControl_Soft,, "&H2&I2&R1"
HKR, Settings, ErrorControl_On,, "&M4"
HKR, Settings, ErrorControl_Off,, "&M0"
HKR, Settings, ErrorControl_Forced,, "&M5"
HKR, Settings, Compression_On,, "&K1"
HKR, Settings, Compression_Off,, "&K0"
HKR, Settings, Modulation_CCITT,, "B0"
HKR, Settings, Modulation_Bell,,  "B1"
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
HKR, Settings, Blind_Off,, "X2"
HKR, Settings, Blind_On,, "X0"
HKR, Settings, CallSetupFailTimer,, "S7=<#>"
; HKR, Settings, InactivityTimeout,, "S19=<#>"

HKR,Responses,"<cr><lf>BUSY<cr><lf>",1,06,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>ERROR<cr><lf>",1,03,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>NO ANSWER<cr><lf>",1,07,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>NO CARRIER<cr><lf>",1,04,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>NO DIAL TONE<cr><lf>",1,05,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>OK<cr><lf>",1,00,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>RING<cr><lf>",1,08,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>RINGING<cr><lf>",1,01,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT<cr><lf>",1,02,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28400<cr><lf>",1,02,00,F0,6E,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000<cr><lf>",1,02,00,00,7D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000/ARQ<cr><lf>",1,02,00,00,7D,00,00,00,00,00,00

[Verbose]
HKR, Responses, "<cr>",        1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<lf>",        1, 01, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "0<cr>",       1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK
HKR, Responses, "2<cr>",       1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING
HKR, Responses, "3<cr>",       1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER
HKR, Responses, "4<cr>",       1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR
HKR, Responses, "6<cr>",       1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE
HKR, Responses, "7<cr>",       1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY
HKR, Responses, "8<cr>",       1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER

; [Fast]
; HKR, Init, 2,, "AT&F1&B1&C1&D2E0Q0V1&A3S0=0<cr>"


