tab li24

# Li-24/Hart / APT-2000ALW

It contains additional transmitter parameters. Description of individual fields can be found in the product’s valid Operation and Maintenance Manual.

The first tab allows to set the following parameters:

1. Input type
2. Range
3. Connection type
4. Additional parameters

The second tab allows to set the following parameters:

1. Measurement type
2. Electric current configuration. Namur mode field

- checked
- alarm current compliant with NAMUR.
- unchecked
- Normal mode. Electric current values described in OM Manual.

3. Alarms
4. Alarm current

Content of fields, in which value can be entered, can be transfered to the transmitter with a command Write parameters.
The command Read parameters allows to read only those parameters, which are shown in the above window.
To read all transmitter parameters, you should use the command Read configuration.